* Define pin TX ca si output si pin RX ca si input
* <https://dronebotworkshop.com/getting-started-with-lidar/>

The problem with XCP is under investigation by the Mathworks support team.

New features added for exe file:

\* Pop-up error message, for the end user (to see if the application has some errors).

\* Create a log file when an error occurs, for us to investigate possible issues.